# ECP5-5G LUT library for ABC
# Note that ECP5 architecture assigns difference
# in LUT input delay to interconnect, so this is
# considered too


# Simple LUTs
#  area  D    C    B    A
1  1     141
2  1     141  275
3  1     141  275  379
4  1     141  275  379  379
