# 512 x 40 bit -> CC_BRAM_20K SDP RAM
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 9 -set DATA_WIDTH 40 sync_ram_sdp
synth_gatemate -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:CC_BUFG
select -assert-count 1 t:CC_BRAM_20K

# 512 x 20 bit x 2 -> CC_BRAM_20K TDP RAM
design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 9 -set DATA_WIDTH 20 sync_ram_tdp
synth_gatemate -top sync_ram_tdp -noiopad
select -assert-count 2 t:CC_BUFG
select -assert-count 1 t:CC_BRAM_20K

# 512 x 80 bit -> CC_BRAM_40K SDP RAM
design -reset
read_verilog ../common/blockram.v
chparam -set ADDRESS_WIDTH 9 -set DATA_WIDTH 80 sync_ram_sdp
synth_gatemate -top sync_ram_sdp -noiopad
cd sync_ram_sdp
select -assert-count 1 t:CC_BUFG
select -assert-count 1 t:CC_BRAM_40K

# 512 x 40 bit -> CC_BRAM_20K SDP ROM
design -reset
read_verilog ../common/blockrom.v
chparam -set ADDRESS_WIDTH 9 -set DATA_WIDTH 40 sync_rom
synth_gatemate -top sync_rom -noiopad
cd sync_rom
select -assert-count 1 t:CC_BUFG
select -assert-count 1 t:CC_BRAM_20K

# 512 x 80 bit -> CC_BRAM_40K SDP ROM
design -reset
read_verilog ../common/blockrom.v
chparam -set ADDRESS_WIDTH 9 -set DATA_WIDTH 80 sync_rom
synth_gatemate -top sync_rom -noiopad
cd sync_rom
select -assert-count 1 t:CC_BUFG
select -assert-count 1 t:CC_BRAM_40K
