read_verilog ../common/mul.v
chparam -set X_WIDTH 8 -set Y_WIDTH 8 -set A_WIDTH 16
hierarchy -top top
proc
equiv_opt -assert -map +/intel_alm/common/dsp_sim.v synth_intel_alm -family cyclonev -noiopad -noclkbuf # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd top # Constrain all select calls below inside the top module

select -assert-count 1 t:MISTRAL_MUL9X9
select -assert-none t:MISTRAL_MUL9X9 %% t:* %D

# Cyclone 10 GX does not have 9x9 multipliers.

design -reset
read_verilog ../common/mul.v
chparam -set X_WIDTH 17 -set Y_WIDTH 17 -set A_WIDTH 34
hierarchy -top top
proc
equiv_opt -assert -map +/intel_alm/common/dsp_sim.v synth_intel_alm -family cyclonev -noiopad -noclkbuf # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd top # Constrain all select calls below inside the top module

select -assert-count 1 t:MISTRAL_MUL18X18
select -assert-none t:MISTRAL_MUL18X18 %% t:* %D

design -reset
read_verilog ../common/mul.v
chparam -set X_WIDTH 17 -set Y_WIDTH 17 -set A_WIDTH 34
hierarchy -top top
proc
equiv_opt -assert -map +/intel_alm/common/dsp_sim.v synth_intel_alm -family cyclone10gx -noiopad -noclkbuf # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd top # Constrain all select calls below inside the top module

select -assert-count 1 t:MISTRAL_MUL18X18
select -assert-none t:MISTRAL_MUL18X18 %% t:* %D

design -reset
read_verilog ../common/mul.v
chparam -set X_WIDTH 26 -set Y_WIDTH 26 -set A_WIDTH 52
hierarchy -top top
proc
equiv_opt -assert -map +/intel_alm/common/dsp_sim.v synth_intel_alm -family cyclonev -noiopad -noclkbuf # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd top # Constrain all select calls below inside the top module

select -assert-count 1 t:MISTRAL_MUL27X27
select -assert-none t:MISTRAL_MUL27X27 %% t:* %D

design -reset
read_verilog ../common/mul.v
chparam -set X_WIDTH 26 -set Y_WIDTH 26 -set A_WIDTH 52
hierarchy -top top
proc
equiv_opt -assert -map +/intel_alm/common/dsp_sim.v synth_intel_alm -family cyclone10gx -noiopad -noclkbuf # equivalency check
design -load postopt # load the post-opt design (otherwise equiv_opt loads the pre-opt design)
cd top # Constrain all select calls below inside the top module

select -assert-count 1 t:MISTRAL_MUL27X27
select -assert-none t:MISTRAL_MUL27X27 %% t:* %D
